Supplementary Figure S1: A - Number of TAD values obtained between 0.5 and 1.0 for each value of S (vertical travel speed), here for seal B09, and B – corresponding derivative of this number of 0.5<TAD <1.0 for each S value. The chosen speed S here is 1.8 m.s-1, when the second derivative reaches zero.



